Marlin WebUI by atbox.tech
Disconnected
Printer status
Printing status
Idle
Printing timer
Remain: 0:45:12
Estimated: 1:12:34
Elapsed: 0:00:00
Printing progress:
10%
1 of 123456
Temperatures
Auto temperature detection

Sensor
Hotend (extruder) sensor
Bed sensor
| Detected
-
-
| Set
-
-
| Unit
-
-
| Chart display
Show
Show

Hotend fan speed

Current fan speed | -
Set fan speed | -
OFF | 10% | 20% | 30% | 40% | 50% | 60% | 70% | 80% | 90% | FULL

Home positioning

All axis |  | X axis |  | Y axis |  | Z axis

Movements
Steps movements size (mm)
Move on X axis
Move on Y axis
Move on Z axis
Steppers locking

Lock/Unlock all steppers (X, Y, Z, E) |
X stepper |  | Y stepper |  | Z stepper |  | E stepper

Filament
Upload...
Choose file

Filename (DOS8 Format) - | File size - | G-Code Lines -

File processing

SD Content management
Selected file:
Files:
0
Folders:
0
SD File list
G-Code command:
G-Code checksum value:
Console output:

Info...
Marlin WebUI

Release date: January, 1 2020

Github project: E4d-box-project
Facebook: E4d@box

Open source dependencies:

- Marlin firmware
- JQuery 3.5.1 (slim version)
- Bootstrap v4.5.0
- Bootstrap4 toggle switch v3.6.1
- Fontastic
- Chart.js
- FileSaver.js

Settings..

- Auto connect:
  If ON the application will try to connect automatically on start
- Temp interval:
  Set the default temperature detection interval (secs)
- Temp unit:
  Set the default temperature unit
- Default panel:
  Set the default shown panel on start
- Trace direction:
  Append Prepend
  Set the console trace direction
- Trace symbol
  Set the console message direction symbol
- Logging level
  Set the JavaScript logging level

Settings saved successfully
GCommand presets
- Replace {N} chars with the specific parameter that you need if present (ie: G1 X{0} => G1 X10)
Connect...
Ooopsss!
Marlin firmware Web Socket is not connected.
Would you like connect it now?
Deletion confirmation
Are you sure to delete
SD card file?
This operation cannot be undone.
File deleted successfully
Print confirmation
Are you sure to start printing of
Printing started successfully
Message